General idea:

* A script is written using [Ducky scripting language 1.0](https://web.archive.org/web/20220816200129/http://github.com/hak5darren/USB-Rubber-Ducky/wiki/Duckyscript) and additional commands from [flipper](https://docs.flipperzero.one/bad-usb) that emulates a keyboard to quickly perform tasks on the victim’s computer.

Inspiration: badUSB script to open a web page

DEFAULT\_DELAY 500

GUI r

STRING powershell Start-Process\ "https://www.youtube.com/watch?v=wFCJVy-vM7o"

ENTER

Some Commands: More in the General Idea links

REM Comment

GUI Windows key

DELAY n sleep n milliseconds

DEFAULT\_DELAY set a default time between commands

STRING types the text following

APP app menu, same as shift - F10

SHIFT optional extra parameters: see Ducky 1.0

ALT optional extra parameters: see Ducky 1.0

CTRL optional extra parameters: see Ducky 1.0

DOWN arrow key

LEFT arrow key

RIGHT arrow key

UP arrow key

REPEAT n repeat last command n times